# EESACZ Lines

Shapefile

Thumbnail Not Available

Tags
Water Body, Pond, Waterbodies, environment, Hydrography, Ponds, Waterbody, Lakes Water Bodies, Reservior, Lake, Streams, Rivers, California, inlandWaters

Summary

    This dataset was derived by intersecting the National Hydrography Dataset (NHD) high resolution flowlines features of California with the boundaries of the San Francisco Bay Conservation and Development Commission (BCDC) and California Coastal Commission (CCC).

Description

                        To provide owners and operators of Inland Facilities, Oil Spill preparers, and plan reviewers with definition and tools needed to identify waters of the state within the CCC and BCDC boundaries for purposes of determining oil spill contingency planning requirements for Inland Facilities.

Credits

    San Francisco Bay Conservation and Development Commission (BCDC), California Coastal Commission (CCC), and California Department of Fish and Wildlife, Office of Spill Prevention and Response (CDFW-OSPR)

Use limitations

There are no access and use limitations for this item.

Extent

West | -124.582703 | East | -112.165770
North | 43.346753 | South | 32.345044

Scale Range

Maximum (zoomed in) | 1:5,000
Minimum (zoomed out) | 1:150,000,000

## ArcGIS Metadata ▼►

## Topics and Keywords ▼►

Themes or categories of the resourceenvironment, inlandWaters
* Content typeDownloadable Data

Export to FGDC CSDGM XML format as Resource DescriptionNo

Place keywordsCalifornia

Theme keywordsWater Body, Pond, Waterbodies, Hydrography, Ponds, Waterbody, Lakes, Water Bodies, Reservior, Lake, Streams, Rivers

Hide Topics and Keywords ▲

## Citation ▼►

TitleEESACZ Lines
Creation date2016-10-24 00:00:00
Publication date2016-10-24 00:00:00
Presentation formatsdigital map
FGDC geospatial presentation formatvector digital data
Collection titleState Waters Within BCDC Boundary
Hide Citation ▲

## Resource Details ▼►

Dataset languagesEnglish (UNITED STATES)
Dataset character setutf8 - 8 bit UCS Transfer Format
Statuscompleted
Spatial representation typevector
Processing environmentMicrosoft Windows 7 Version 6.1 (Build 7601) Service Pack 1; Esri ArcGIS 10.3.1.4959
Credits

      San Francisco Bay Conservation and Development Commission (BCDC), California Coastal Commission (CCC), and California Department of Fish and Wildlife, Office of Spill Prevention and Response (CDFW-OSPR)

ArcGIS item properties

* NameEESACZ_Lines
* Size16.635
* Locationfile://\\geodata.ad.dfg.ca.gov\GIS\OSPR_GIS\Projects\Work_in_Progress\GEwing\Projects\2016\Judd_Muskat\State_Fire_Marshall\Datasets\Round3_EESA\Shp\EESACZ_Lines.shp

* Access protocolLocal Area Network

Hide Resource Details ▲

## Extents ▼►

Extent

Geographic extent

Bounding rectangle

Extent typeExtent used for searching
West longitude-124.582703
East longitude-112.165770
North latitude43.346753
South latitude32.345044
Extent contains the resourceYes

Extent in the item's coordinate system

* West longitude-124.403593
* East longitude-116.535416
* South latitude32.536509
* North latitude42.007632
* Extent contains the resourceYes

Hide Extents ▲

## Resource Points of Contact ▼►

Point of contact

Individual's nameGreg Ewing
Organization's nameCalifornia Department of Fish and Wildlife, Office of Spill Prevention and Response (CDFW - OSPR)
Contact's positionGIS Analyst
Contact's rolepoint of contact

Contact information ▼►

Phone

Voice916-327-9962

Address

Typeboth
Delivery point1700 K Street, Ste 250
CitySacramento
Administrative areaCA
Postal code95811
CountryUS
e-mail address Greg.Ewing@wildlife.ca.gov

Hide Contact information ▲

Hide Resource Points of Contact ▲

## Resource Maintenance ▼►

Resource maintenance

Update frequencyas needed

Hide Resource Maintenance ▲

## Spatial Reference ▼►

ArcGIS coordinate system

* TypeGeographic
* Geographic coordinate referenceGCS_WGS_1984
* Coordinate reference details

Geographic coordinate system

Well-known identifier4326
X origin-400
Y origin-400
XY scale11258999068426.238
Z origin-100000
Z scale10000
M origin-379228.81179800001
M scale8192000003.8146954
XY tolerance8.983152841195215e-009
Z tolerance0.001
M tolerance0.001
High precisiontrue
Left longitude-180
Latest well-known identifier4326
Well-known textGEOGCS["GCS_WGS_1984",DATUM["D_WGS_1984",SPHEROID["WGS_1984",6378137.0,298.257223563]],PRIMEM["Greenwich",0.0],UNIT["Degree",0.0174532925199433],AUTHORITY["EPSG",4326]]

Reference system identifier

Value3310
CodespaceEPSG
Version8.6.2

Hide Spatial Reference ▲

## Spatial Data Properties ▼►

Vector ▼►

* Level of topology for this datasetgeometry only
Geometric objects

Feature class nameEESACZ_Lines
* Object typecomposite
* Object count8281

Hide Vector ▲
ArcGIS Feature Class Properties
▼ ►

Feature class nameEESACZ_Lines

* Feature typeSimple
* Geometry typePolyline
* Has topologyFALSE
* Feature count8281
* Spatial indexTRUE
* Linear referencingTRUE

Hide ArcGIS Feature Class Properties ▲
Hide Spatial Data Properties ▲

## Data Quality ▼►

Scope of quality information ▼►

Resource leveldataset

Hide Scope of quality information ▲
Hide Data Quality ▲

## Geoprocessing history ▼►

Process

Process name
Date2015-09-11 11:59:01
Tool locationc:\program files (x86)\arcgis\desktop10.1\ArcToolbox\Toolboxes\Analysis Tools.tbx\Clip
Command issued

Clip CA_Streams_2_Statewide cnty24k09_1_state_poly T:\OSPR_Data\Ospr_GIS_Lib\Projects_Groups_Misc\ERMA_files\ERMA_Shp_WGS84\Bathymetry_Hydrology\Hydrology_Hydrography\SurfaceWaters_California\CA_Streams_NHD\All_CA_Streams_Statewide.shp #

Include in lineage when exporting metadataNo

Process

Process name
Date2016-02-09 15:39:46
Tool locationc:\program files (x86)\arcgis\desktop10.1\ArcToolbox\Toolboxes\Data Management Tools.tbx\Project
Command issued

Project T:\OSPR_Data\Ospr_GIS_Lib\Projects_Groups_Misc\ERMA_files\ERMA_Shp_WGS84\Bathymetry_Hydrology\Hydrology_Hydrography\CA_SurfaceWaters\All_CA_Streams_NHD\All_CA_Streams_Statewide_Clipped_TA83.shp T:\OSPR_Data\Ospr_GIS_Lib\Projects_Groups_Misc\ERMA_files\ERMA_Shp_WGS84\Bathymetry_Hydrology\Hydrology_Hydrography\CA_SurfaceWaters\All_CA_Streams_NHD\All_CA_Streams_Statewide.shp GEOGCS['GCS_WGS_1984',DATUM['D_WGS_1984',SPHEROID['WGS_1984',6378137.0,298.257223563]],PRIMEM['Greenwich',0.0],UNIT['Degree',0.0174532925199433],METADATA['World',-180.0,-90.0,180.0,90.0,0.0,0.0174532925199433,0.0,1262]] WGS_1984_(ITRF00)_To_NAD_1983 PROJCS['NAD_1983_California_Teale_Albers',GEOGCS['GCS_North_American_1983',DATUM['D_North_American_1983',SPHEROID['GRS_1980',6378137.0,298.257222101]],PRIMEM['Greenwich',0.0],UNIT['Degree',0.0174532925199433]],PROJECTION['Albers'],PARAMETER['False_Easting',0.0],PARAMETER['False_Northing',-4000000.0],PARAMETER['Central_Meridian',-120.0],PARAMETER['Standard_Parallel_1',34.0],PARAMETER['Standard_Parallel_2',40.5],PARAMETER['Latitude_Of_Origin',0.0],UNIT['Meter',1.0]]

Include in lineage when exporting metadataNo

Process

Process name
Date2016-11-23 07:25:03
Tool locationc:\program files (x86)\arcgis\desktop10.4\ArcToolbox\Toolboxes\Data Management Tools.tbx\Merge
Command issued

Merge StateWaters_BCDC_Jurisdiction;StateWaters_CoastalZone C:\Users\elevy\Desktop\OSPR\OSPR_EESACZ.gdb\EESACZ_Lines "Name "Name" true true false 65 Text 0 0 ,First,#,StateWaters_BCDC_Jurisdiction,Name,-1,-1,StateWaters_CoastalZone,Name,-1,-1;DFGWATERID "DFGWATERID" true true false 10 Long 0 10 ,First,#,StateWaters_BCDC_Jurisdiction,DFGWATERID,-1,-1,StateWaters_CoastalZone,DFGWATERID,-1,-1;Mouth_Lat "Mouth_Lat" true true false 19 Double 0 0 ,First,#,StateWaters_BCDC_Jurisdiction,Mouth_Lat,-1,-1,StateWaters_CoastalZone,Mouth_Lat,-1,-1;Mouth_Long "Mouth_Long" true true false 19 Double 0 0 ,First,#,StateWaters_BCDC_Jurisdiction,Mouth_Long,-1,-1,StateWaters_CoastalZone,Mouth_Long,-1,-1;Down_Name "Down_Name" true true false 100 Text 0 0 ,First,#,StateWaters_BCDC_Jurisdiction,Down_Name,-1,-1,StateWaters_CoastalZone,Down_Name,-1,-1;Down_ID "Down_ID" true true false 10 Long 0 10 ,First,#,StateWaters_BCDC_Jurisdiction,Down_ID,-1,-1,StateWaters_CoastalZone,Down_ID,-1,-1;Mouth_Meas "Mouth_Meas" true true false 10 Long 0 10 ,First,#,StateWaters_BCDC_Jurisdiction,Mouth_Meas,-1,-1,StateWaters_CoastalZone,Mouth_Meas,-1,-1;Source_Mea "Source_Mea" true true false 19 Double 0 0 ,First,#,StateWaters_BCDC_Jurisdiction,Source_Mea,-1,-1,StateWaters_CoastalZone,Source_Mea,-1,-1;EditVersio "EditVersio" true true false 5 Long 0 5 ,First,#,StateWaters_BCDC_Jurisdiction,EditVersio,-1,-1,StateWaters_CoastalZone,EditVersio,-1,-1;EditNotes "EditNotes" true true false 254 Text 0 0 ,First,#,StateWaters_BCDC_Jurisdiction,EditNotes,-1,-1,StateWaters_CoastalZone,EditNotes,-1,-1;EventAlert "EventAlert" true true false 5 Text 0 0 ,First,#,StateWaters_BCDC_Jurisdiction,EventAlert,-1,-1,StateWaters_CoastalZone,EventAlert,-1,-1;GNIS_ID "GNIS_ID" true true false 10 Text 0 0 ,First,#,StateWaters_BCDC_Jurisdiction,GNIS_ID,-1,-1,StateWaters_CoastalZone,GNIS_ID,-1,-1;NHD_Perman "NHD_Perman" true true false 40 Text 0 0 ,First,#,StateWaters_BCDC_Jurisdiction,NHD_Perman,-1,-1,StateWaters_CoastalZone,NHD_Perman,-1,-1;Alternate_ "Alternate_" true true false 100 Text 0 0 ,First,#,StateWaters_BCDC_Jurisdiction,Alternate_,-1,-1,StateWaters_CoastalZone,Alternate_,-1,-1;Enabled "Enabled" true true false 5 Long 0 5 ,First,#,StateWaters_BCDC_Jurisdiction,Enabled,-1,-1,StateWaters_CoastalZone,Enabled,-1,-1"

Include in lineage when exporting metadataNo

Process

Process name
Date2016-11-23 07:29:00
Tool locationc:\program files (x86)\arcgis\desktop10.4\ArcToolbox\Toolboxes\Data Management Tools.tbx\DeleteField
Command issued

DeleteField EESACZ_Lines Name;DFGWATERID;Mouth_Lat;Mouth_Long;Down_Name;Down_ID;Mouth_Meas;Source_Mea;EditVersio;EditNotes;EventAlert;GNIS_ID;NHD_Perman;Alternate_;Enabled

Include in lineage when exporting metadataNo

Hide Geoprocessing history ▲

## Distribution ▼►

Distribution format

NameShapefile

Transfer options

* Transfer size16.635

Hide Distribution ▲

## Fields ▼►

Details for object EESACZ_Lines ▼►

* TypeFeature Class
* Row count8281
Field FID
▼►

* AliasFID
* Data typeOID
* Width4
* Precision0
* Scale0
* Field description

      Internal feature number.

* Description source

      Esri

* Description of values

      Sequential unique whole numbers that are automatically generated.

Hide Field FID ▲
Field Shape
▼►

* AliasShape
* Data typeGeometry
* Width0
* Precision0
* Scale0
Field description

      Feature geometry.

Description source

      ESRI

Description of values

      Coordinates defining the features.

Hide Field Shape ▲
Field Shape_Leng
▼►

* AliasShape_Leng
* Data typeDouble
* Width19
* Precision0
* Scale0

Hide Field Shape_Leng ▲

Hide Details for object EESACZ_Lines ▲
Hide Fields ▲

## Metadata Details ▼►

Metadata languageEnglish (UNITED STATES)
Metadata character setutf8 - 8 bit UCS Transfer Format
Scope of the data described by the metadatadataset
Scope namedataset
Last update2015-09-09
ArcGIS metadata properties

Metadata formatArcGIS 1.0
Standard or profile used to edit metadataFGDC
Metadata styleFGDC CSDGM Metadata
Created in ArcGIS for the item2016-12-14 10:36:28
Last modified in ArcGIS for the item2016-12-15 15:19:33
Automatic updates

Have been performedYes
Last update2016-12-15 15:19:33

Hide Metadata Details ▲

## Metadata Maintenance ▼►

Maintenance

Update frequencyas needed

Hide Metadata Maintenance ▲

## FGDC Metadata (read-only) ▼►

## Identification ▼►

  Citation
    Citation Information
      Originator CDFW Biogeographic Data Section with CDFW Northern Region Data Management and GIS
      Publication Date February 2014
      Title
        California Streams (CA_Streams_2)
      Geospatial Data Presentation Form vector digital data
  Description
    Abstract

                                      National Hydrography Dataset (NHD) high resolution NHDFlowline features for California were originally dissolved on common GNIS_ID or StreamLevel* attributes and routed from mouth to headwater in meters. The results are measured polyline features representing entire streams. Routes on these streams are measured upstream, i.e., the measure at the mouth of a stream is zero and at the upstream end the measure matches the total length of the stream feature. Using GIS tools, a user of this dataset can retrieve the distance in meters upstream from the mouth at any point along a stream feature.** *See the Source Citation section of this metadata for further information on NHD, NHDFlowline, GNIS_ID and StreamLevel. **See the Data Quality section of this metadata for further explanation of stream feature development. CA_Streams_v2x Update Notes: This version includes hundreds of stream modifications and additions resulting from requests for updating from CDFW staff and others as well as some updates included in the current USGS NHD dataset***. Stream edits and additions tracking and editor notes are available in new attribute fields 'EditVersion' and 'EditNotes.' In addition, for users that have indexed data to the older version of CA_Streams, 'EditNotes' attempts to describe how the edit has affected the indexed measure values on the edited streams. Also, 'EventAlert' attributes provide a quick way to query for streams where editing has affected previously indexed data. New value added attributes have been included in v2, including 'Down_Name' and 'Down_ID' which provide the CA_Stream DFGWATERID and GNIS_Name (if applicable) of the stream's downstream parent (i.e., "Tributary to")****. These attributes can aid the user in locating a stream that might share its name with several streams throughout California for example. An 'Alternate_Name' attribute field has been added for users in their area of interest to record stream names that might be different or not included in GNIS (USGS Geographic Names Information System). This version has also been configured to be geometric network ready. Advanced users may now be able to create a geometric network to enable downstream and upstream tracing and utilize the new 'Enabled' attribute to enable or disable tracing on any given stream. More information on geometric networking can be found online at ESRI arcgis.com. ***Some current NHD data has not yet been included in CA_Streams. The effort to synchronize CA_Streams with NHD is ongoing. ****Some streams have more than one downstream parent, but the attributes in this dataset can only include one of those parents (the named parent is included if applicable). Please email the point of contact for this dataset for a table including all downstream parents.

    Purpose

                                      To provide an alternative to the native NHD measuring system of percentage of distance along reach length with one that enhances the ability to examine distance relationships along entire stream courses.

  Time Period of Content
    Currentness Reference

                                      publication date

  Status
    Progress In work
    Maintenance and Update Frequency As needed
  Spatial Domain
    Bounding Coordinates
      West Bounding Coordinate -124.253043
      East Bounding Coordinate -123.617226
      North Bounding Coordinate 42.148970
      South Bounding Coordinate 41.501444
  Keywords
    Theme
      Theme Keyword whole stream
      Theme Keyword route
      Theme Keyword stream
      Theme Keyword meters
      Theme Keyword stream based
      Theme Keyword complex edge
      Theme Keyword measured
  Access Constraints

                                none

  Use Constraints

                                none

  Point of Contact
    Contact Information
      Contact Person Primary
        Contact Person Tom Christy
        Contact Organization California Department of Fish and Wildlife Northern Region Data Management and GIS
      Contact Position GIS Analyst
      Contact Voice Telephone 530-225-2276
      Contact Electronic Mail Address Tom.Christy@wildlife.ca.gov
  Native Data Set Environment
    Microsoft Windows XP Version 5.1 (Build 2600) Service Pack 3; ESRI ArcCatalog 9.3.1.3500

Hide Identification ▲

## Data Quality ▼►

  Attribute Accuracy
    Attribute Accuracy Report

                                      CA_Streams are roiginally based on NHDFlowline feature geometry, GNIS_ID attributes and StreamLevel attributes.* When not provided by NHD, StreamLevel attributes were calculated using the NHD PGDB Releveler tool, a tool provided by NHD to trained NHD editors.

          *Many NHDFlowline features, including but not exclusive to canal and ditch features, are not included in this dataset due to problems with the interpretation of streams from such features. Some NHDFlowline features as indicated in 'EditVersion' attributes as having been modified by DFW projects and programs prior to routing as streams, are planned to but have not yet been submitted to NHD. See 'EditNotes' attributes for descriptions of these edits or email this dataset's point contact for additional information.

  Lineage
    Source Information
      Source Citation
        Citation Information
          Originator USGS National Hydrography Dataset
          Title
            Stream Level Documentation
          Other Citation Details
            page 18 (see online linkage below)
          Online Linkage http://nhd.usgs.gov/chapter1/chp1_data_users_guide.pdf
    Source Information
      Source Citation
        Citation Information
          Originator USGS National Hydrography Dataset
          Title
            PGDB Releveler tool
          Other Citation Details
            PGDbReleveler Version 2.2.1 Designed and developed by Horizon Systems Corporation under contract to the U.S. Environmental Protection Agency Office of Water - Office of Wetlands, Oceans, and Watersheds in cooperation with the U.S. Geological Survey. For more information please email info@horizon-system.com or Call (703) 471-0480. Purpose: PGDbReleveler is designed to recalculate the Streamlevel field in the NHDflowlineVAA table of an ESRI/NHD Personal GeoDatabase. Input: A valid ESRI/NHD Personal GeoDatabase with a logically correct NHDflow table. Output: A releveled ESRI/NHD Personal GeoDatabase. A cumulative log file (PGDbReleveler.log) is created/updated after each run with the results of the last relevel process.
    Source Information
      Source Citation
        Citation Information
          Originator U.S. Geological Survey in cooperation with U.S. Environmental Protection Agency, USDA Forest Service, and other Federal, State and local partners
          Publication Date Varies per feature
          Title
            National Hydrography Dataset (NHD)
          Other Citation Details
            The National Hydrography Dataset (NHD) is a feature-based database that interconnects and uniquely identifies the stream segments or reaches that make up the nation's surface water drainage system. NHD data was originally developed at 1:100,000-scale and exists at that scale for the whole country. This high-resolution NHD, generally developed at 1:24,000/1:12,000 scale, adds detail to the original 1:100,000-scale NHD. (Data for Alaska, Puerto Rico and the Virgin Islands was developed at high-resolution, not 1:100,000 scale.) Local resolution NHD is being developed where partners and data exist. The NHD contains reach codes for networked features, flow direction, names, and centerline representations for areal water bodies. Reaches are also defined on waterbodies and the approximate shorelines of the Great Lakes, the Atlantic and Pacific Oceans and the Gulf of Mexico. The NHD also incorporates the National Spatial Data Infrastructure framework criteria established by the Federal Geographic Data Committee. Addendum: Modifications made by DFG to NHD Flowlines (reaches) for the purpose of enabling/enhancing DFG programs and projects have been included in this feature class. A field named DFG_Edit has been added to the attribute table to provide a description of these modifications. Only records with an entry in DFG_Edit have been modified from the original NHDFlowline feature class, hence these modifications have not yet been submitted to NHD.
          Online Linkage http://nhd.usgs.gov/ or http://nhd.usgs.gov/chapter1/chp1_data_users_guide.pdf
    Source Information
      Source Citation
        Citation Information
          Originator US Geological Survey
          Publication Date Ongoing
          Title
            Geographic Names Information System (GNIS)
          Other Citation Details
            The Geographic Names Information System (GNIS), developed by the U.S. Geological Survey in cooperation with the U.S. Board on Geographic Names, contains information about physical and cultural geographic features in the United States and associated areas, both current and historical (not including roads and highways). The database holds the Federally recognized name of each feature and defines the location of the feature by state, county, USGS topographic map, and geographic coordinates.
          Online Linkage http://nhd.usgs.gov/gnis.html

Hide Data Quality ▲

## Spatial Reference ▼►

  Horizontal Coordinate System Definition
    Geodetic Model
      Horizontal Datum Name North American Datum of 1983
      Ellipsoid Name Geodetic Reference System 80
      Semi-major Axis 6378137.000000
      Denominator of Flattening Ratio 298.257222
  Vertical Coordinate System Definition
    Altitude System Definition
      Altitude Resolution 0.000100
      Altitude Encoding Method Explicit elevation coordinate included with horizontal coordinates

Hide Spatial Reference ▲

## Entities and Attributes ▼►

  Detailed Description
    Entity Type
      Entity Type Label CA_Streams_2_Statewide
    Attribute
      Attribute Label FID
      Attribute Definition
        Internal feature number.
      Attribute Definition Source Esri
      Attribute Domain Values
        Unrepresentable Domain
          Sequential unique whole numbers that are automatically generated.
    Attribute
      Attribute Label Shape
      Attribute Definition
        Feature geometry.
      Attribute Definition Source ESRI
      Attribute Domain Values
        Unrepresentable Domain
          Coordinates defining the features.
    Attribute
      Attribute Label Shape_Leng

Hide Entities and Attributes ▲

## Distribution Information ▼►

  Resource Description Downloadable Data
  Standard Order Process
    Digital Form
      Digital Transfer Information
        Transfer Size 0.000

Hide Distribution Information ▲

## Metadata Reference ▼►

  Metadata Date February 2014
  Metadata Contact
    Contact Information
      Contact Person Primary
        Contact Person Tom Christy
        Contact Organization California Department of Fish and Wildlife Northern Region Data Management and GIS
      Contact Position GIS Analyst
      Contact Address
        Address Type REQUIRED: The mailing and/or physical address for the organization or individual.
        City REQUIRED: The city of the address.
        State or Province REQUIRED: The state or province of the address.
        Postal Code REQUIRED: The ZIP or other postal code of the address.
      Contact Voice Telephone 530_225-2276
      Contact Electronic Mail Address Tom.Christy@wildlife.ca.gov
  Metadata Standard Name FGDC Content Standards for Digital Geospatial Metadata
  Metadata Standard Version FGDC-STD-001-1998
  Metadata Time Convention local time

Hide Metadata Reference ▲