# Public Land Survey System (All Areas Filled, Includes Protracted Data) (100K Source)

Shapefile

Thumbnail Not Available

Tags
ranges, landgrants, boundaries, planningCadastre, townships, TRS, grids, PLSS, sections, Public Land Survey System, PLS, California

Summary

    To display and analyze township, range, and sections as contained in the Public Land Survey System grid.

Description

    This layer differs from the standard Public Land Survey System layer in that all landgrants and other areas excluded from the section survey process are filled in (with protracted data). The primary purpose of this is to facilitate the georeferencing of phenomena that are spatially referenced by meridian, township, range, and section. Though these sections do not legally exist, field personnel will interpolate to determine what the section would be if there were legally a section there. This is common with fire starts as reported by the California Department of Forestry (CDF). In fact, all of the work to fill in these excluded areas was completed by CDF to help georeference fire starts so they could be analyzed with GIS (Geographic Information Systems) technology. This layer is based on 1:100,000-scale (100K) source data. Caution should be used when attempting to use it with more detailed sources such as 1:24,000-scale (24K) data. For the most current and detailed PLSS data, users should refer to BLM's Geographic Coordinate Data Base (GCDB). This layer depicts the township, range and sections contained in the Public Land Survey System grid for the State of California. Townships are roughly six miles square, and are numbered north and south from an established baseline. Likewise, ranges are numbered east and west from an established meridian. California uses three baseline/meridians, these being Humboldt, Mt. Diablo, and San Bernardino, abbreviated H, M, and S Meridian, township, range, and section values are combined in the redefined item MTRS to facilitate relates from/to other tables.

Credits

There are no credits for this item.

Use limitations

There are no access and use limitations for this item.

Extent

West | -124.506055 | East | -113.498654
North | 42.068938 | South | 32.423519

Scale Range
There is no scale range for this item.

## ArcGIS Metadata ▼►

## Topics and Keywords ▼►

Themes or categories of the resourceplanningCadastre, boundaries
Content typeDownloadable Data
Place keywordsCalifornia

Theme keywordsranges, landgrants, boundaries, planningCadastre, townships, TRS, grids, PLSS, sections, Public Land Survey System, PLS

Hide Topics and Keywords ▲

## Citation ▼►

TitlePublic Land Survey System (All Areas Filled, Includes Protracted Data) (100K Source)
Publication date

Indeterminate dateunknown

Presentation formats *digital map
Hide Citation ▲

## Citation Contacts ▼►

Responsible party

Organization's nameCalifornia Department of Forestry and Fire Protection
Contact's roleoriginator

Responsible party

Organization's nameU.S. Geological Survey
Contact's roleoriginator

Hide Citation Contacts ▲

## Resource Details ▼►

Dataset languagesEnglish (UNITED STATES)
Statuscompleted
Spatial representation type *vector
Supplemental information

      Converted to California Teale Albers NAD83 by the California Department of Fish and Game. Coordinate values also converted to NAD83.

* Processing environmentMicrosoft Windows 7 Version 6.1 (Build 7601) Service Pack 1; Esri ArcGIS 10.5.1.7333
ArcGIS item properties

* NamePLSS_Full_100k
* Size23.806
* Locationfile://\\geodata\GIS\OSPR_GIS\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\PLSS_Full_100k.shp

* Access protocolLocal Area Network

Hide Resource Details ▲

## Extents ▼►

Extent

Geographic extent

Bounding rectangle

Extent typeExtent used for searching
* West longitude-124.506055
* East longitude-113.498654
* North latitude42.068938
* South latitude32.423519
* Extent contains the resourceYes

Extent in the item's coordinate system

* West longitude-373976.200100
* East longitude540014.055800
* South latitude-604525.999100
* North latitude450070.872800
* Extent contains the resourceYes

Hide Extents ▲

## Resource Maintenance ▼►

Resource maintenance

Update frequencynot planned

Hide Resource Maintenance ▲

## Spatial Reference ▼►

ArcGIS coordinate system

* TypeProjected
* Geographic coordinate referenceGCS_North_American_1983
* ProjectionNAD_1983_Albers
* Coordinate reference details

Projected coordinate system

X origin-16909700
Y origin-8597000
XY scale266332319.7555542
Z origin-100000
Z scale10000
M origin-100000
M scale10000
XY tolerance0.001
Z tolerance0.001
M tolerance0.001
High precisiontrue
Well-known textPROJCS["NAD_1983_Albers",GEOGCS["GCS_North_American_1983",DATUM["D_North_American_1983",SPHEROID["GRS_1980",6378137.0,298.257222101]],PRIMEM["Greenwich",0.0],UNIT["Degree",0.0174532925199433]],PROJECTION["Albers"],PARAMETER["False_Easting",0.0],PARAMETER["False_Northing",-4000000.0],PARAMETER["Central_Meridian",-120.0],PARAMETER["Standard_Parallel_1",34.0],PARAMETER["Standard_Parallel_2",40.5],PARAMETER["Latitude_Of_Origin",0.0],UNIT["Meter",1.0]]

Reference system identifier

* Value0

Hide Spatial Reference ▲

## Spatial Data Properties ▼►

Vector ▼►

* Level of topology for this datasetgeometry only
Geometric objects

Feature class namePLSS_Full_100k
* Object typecomposite
* Object count158897

Hide Vector ▲
ArcGIS Feature Class Properties
▼ ►

Feature class namePLSS_Full_100k

* Feature typeSimple
* Geometry typePolygon
* Has topologyFALSE
* Feature count158897
* Spatial indexTRUE
* Linear referencingFALSE

Hide ArcGIS Feature Class Properties ▲
Hide Spatial Data Properties ▲

## Data Quality ▼►

Scope of quality information ▼►

Resource leveldataset

Hide Scope of quality information ▲
Hide Data Quality ▲

## Lineage ▼►

Process step
▼ ►

When the process occurred2007-07-01
Description

      Metadata changes. Noted data as 100K source and added advisory about using BLM GCDB as a more detailed and current PLSS data source.

Process contact

Individual's nameWill Patterson
Organization's nameCalifornia Department of Fish and Game
Contact's roleprocessor

Contact information ▼►

Address

e-mail address geodata@dfg.ca.gov

Hide Contact information ▲

Hide Process step ▲
Process step
▼ ►

When the process occurred2006-01-01
Description

      Metadata edited, noted protracted nature of data.

Process contact

Individual's nameWill Patterson
Organization's nameCalifornia Department of Fish and Game
Contact's roleprocessor

Contact information ▼►

Address

e-mail address geodata@dfg.ca.gov

Hide Contact information ▲

Hide Process step ▲
Process step
▼ ►

When the process occurred2006-09-01
Description

      Misc. edits: 32 features had Township values with control characters as the first character, followed by "06N" - changed to just "06N". 10 features had Township values of "O2N" rather than "02N" - changed to "02N". 7 features had Range values with control characters as the first character, followed by "01W" - changed to "01W". 12 features had Range values "9E" - changed to "09E".

Process contact

Individual's nameJoe Vondracek
Organization's nameCalifornia Department of Fish and Game
Contact's roleprocessor

Contact information ▼►

Address

e-mail address jvondracek@dfg.ca.gov

Hide Contact information ▲

Hide Process step ▲
Hide Lineage ▲

## Geoprocessing history ▼►

Process

Date2018-03-13 15:28:41
Tool locationc:\program files (x86)\arcgis\desktop10.5\ArcToolbox\Toolboxes\Conversion Tools.tbx\FeatureClassToFeatureClass
Command issued

FeatureClassToFeatureClass T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\pls_full.gdb\pls_full_poly T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules PLSS_Full_Poly.shp # "AREA "AREA" true true false 8 Double 0 0 ,First,#,T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\pls_full.gdb\pls_full_poly,AREA,-1,-1;PERIMETER "PERIMETER" true true false 8 Double 0 0 ,First,#,T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\pls_full.gdb\pls_full_poly,PERIMETER,-1,-1;PLS_FULL_ "PLS_FULL_" true true false 4 Long 0 0 ,First,#,T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\pls_full.gdb\pls_full_poly,PLS_FULL_,-1,-1;PLS_FULL_I "PLS_FULL_I" true true false 4 Long 0 0 ,First,#,T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\pls_full.gdb\pls_full_poly,PLS_FULL_ID,-1,-1;MER "MERIDIAN" true true false 1 Text 0 0 ,First,#,T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\pls_full.gdb\pls_full_poly,MER,-1,-1;TOWNSHIP "TOWNSHIP" true true false 5 Text 0 0 ,First,#,T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\pls_full.gdb\pls_full_poly,TOWNSHIP,-1,-1;RANGE "RANGE" true true false 5 Text 0 0 ,First,#,T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\pls_full.gdb\pls_full_poly,RANGE,-1,-1;SECTION "SECTION" true true false 2 Short 0 0 ,First,#,T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\pls_full.gdb\pls_full_poly,SECTION,-1,-1;XALB "XALB" true true false 8 Double 0 0 ,First,#,T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\pls_full.gdb\pls_full_poly,XALB,-1,-1;YALB "YALB" true true false 8 Double 0 0 ,First,#,T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\pls_full.gdb\pls_full_poly,YALB,-1,-1;LATITUDE "LATITUDE" true true false 8 Double 0 0 ,First,#,T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\pls_full.gdb\pls_full_poly,LATITUDE,-1,-1;LONGITUDE "LONGITUDE" true true false 8 Double 0 0 ,First,#,T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\pls_full.gdb\pls_full_poly,LONGITUDE,-1,-1;MTRS "MTRS" true true false 13 Text 0 0 ,First,#,T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\pls_full.gdb\pls_full_poly,MTRS,-1,-1;MTR "MTR" true true false 11 Text 0 0 ,First,#,T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\pls_full.gdb\pls_full_poly,MTR,-1,-1;Shape_Leng "Shape_Length" false true true 8 Double 0 0 ,First,#,T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\pls_full.gdb\pls_full_poly,Shape_Length,-1,-1;Shape_Area "Shape_Area" false true true 8 Double 0 0 ,First,#,T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\pls_full.gdb\pls_full_poly,Shape_Area,-1,-1" #

Include in lineage when exporting metadataNo

Process

Date2018-03-15 13:39:44
Tool locationc:\program files (x86)\arcgis\desktop10.5\ArcToolbox\Toolboxes\Data Management Tools.tbx\Project
Command issued

Project PLSS_Full_100k T:\OSPR_Data\Ospr_GIS_Lib\ERMA\Admin_Boundaries_Reference_Features\Grids_Graticules\PLSS_Full_100k_WGS84.shp GEOGCS['GCS_WGS_1984',DATUM['D_WGS_1984',SPHEROID['WGS_1984',6378137.0,298.257223563]],PRIMEM['Greenwich',0.0],UNIT['Degree',0.0174532925199433]] WGS_1984_(ITRF00)_To_NAD_1983 PROJCS['NAD_1983_Albers',GEOGCS['GCS_North_American_1983',DATUM['D_North_American_1983',SPHEROID['GRS_1980',6378137.0,298.257222101]],PRIMEM['Greenwich',0.0],UNIT['Degree',0.0174532925199433]],PROJECTION['Albers'],PARAMETER['False_Easting',0.0],PARAMETER['False_Northing',-4000000.0],PARAMETER['Central_Meridian',-120.0],PARAMETER['Standard_Parallel_1',34.0],PARAMETER['Standard_Parallel_2',40.5],PARAMETER['Latitude_Of_Origin',0.0],UNIT['Meter',1.0]] NO_PRESERVE_SHAPE # NO_VERTICAL

Include in lineage when exporting metadataNo

Hide Geoprocessing history ▲

## Distribution ▼►

Distributor ▼►

Hide Distributor ▲
Distribution format

* NameShapefile

Transfer options

* Transfer size23.806

Hide Distribution ▲

## Fields ▼►

Details for object PLSS_Full_100k ▼►

* TypeFeature Class
* Row count158897
Field FID
▼►

* AliasFID
* Data typeOID
* Width4
* Precision0
* Scale0
* Field description

      Internal feature number.

* Description source

      Esri

* Description of values

      Sequential unique whole numbers that are automatically generated.

Hide Field FID ▲
Field Shape
▼►

* AliasShape
* Data typeGeometry
* Width0
* Precision0
* Scale0
* Field description

      Feature geometry.

* Description source

      ESRI

* Description of values

      Coordinates defining the features.

Hide Field Shape ▲
Field AREA
▼►

* Width19
* Output width18
* Data typeDouble
* AliasAREA
* Precision0
* Scale0
* Field description

      Area of feature in internal units squared.

* Description source

      ESRI

* Description of values

      Positive real numbers that are automatically generated.

Hide Field AREA ▲
Field PERIMETER
▼►

* Width19
* Output width18
* Data typeDouble
* AliasPERIMETER
* Precision0
* Scale0
* Field description

      Perimeter of feature in internal units.

* Description source

      ESRI

* Description of values

      Positive real numbers that are automatically generated.

Hide Field PERIMETER ▲
Field PLS_FULL_
▼►

* AliasPLS_FULL_
* Data typeInteger
* Width10
* Precision10
* Scale0

Hide Field PLS_FULL_ ▲
Field PLS_FULL_I
▼►

* AliasPLS_FULL_I
* Data typeInteger
* Width10
* Precision10
* Scale0

Hide Field PLS_FULL_I ▲
Field MER
▼►

* AliasMER
* Width1
* Output width1
* Data typeString
* Precision0
* Scale0

Hide Field MER ▲
Field TOWNSHIP
▼►

* Width5
* Output width5
* Data typeString
* AliasTOWNSHIP
* Precision0
* Scale0

Hide Field TOWNSHIP ▲
Field RANGE
▼►

* Width5
* Output width5
* Data typeString
* AliasRANGE
* Precision0
* Scale0

Hide Field RANGE ▲
Field SECTION
▼►

* Width5
* Output width2
* Data typeInteger
* AliasSECTION
* Precision5
* Scale0

Hide Field SECTION ▲
Field XALB
▼►

* Width19
* Output width18
* Data typeDouble
* AliasXALB
* Precision0
* Scale0

Hide Field XALB ▲
Field YALB
▼►

* Width19
* Output width18
* Data typeDouble
* AliasYALB
* Precision0
* Scale0

Hide Field YALB ▲
Field LATITUDE
▼►

* Width19
* Output width18
* Data typeDouble
* AliasLATITUDE
* Precision0
* Scale0

Hide Field LATITUDE ▲
Field LONGITUDE
▼►

* Width19
* Output width18
* Data typeDouble
* AliasLONGITUDE
* Precision0
* Scale0

Hide Field LONGITUDE ▲
Field MTRS
▼►

* Width13
* Output width13
* Data typeString
* AliasMTRS
* Precision0
* Scale0

Hide Field MTRS ▲
Field MTR
▼►

* Width11
* Output width11
* Data typeString
* AliasMTR
* Precision0
* Scale0

Hide Field MTR ▲
Field Shape_Leng
▼►

* AliasShape_Leng
* Data typeDouble
* Width19
* Precision0
* Scale0

Hide Field Shape_Leng ▲
Field Shape_Area
▼►

* AliasShape_Area
* Data typeDouble
* Width19
* Precision0
* Scale0
* Field description

      Area of feature in internal units squared.

* Description source

      Esri

* Description of values

      Positive real numbers that are automatically generated.

Hide Field Shape_Area ▲

Hide Details for object PLSS_Full_100k ▲
Hide Fields ▲

## Metadata Details ▼►

Metadata languageEnglish (UNITED STATES)
Metadata character setutf8 - 8 bit UCS Transfer Format
Scope of the data described by the metadatadataset
Scope name *dataset
* Last update2018-03-13
ArcGIS metadata properties

Metadata formatArcGIS 1.0
Metadata styleFGDC CSDGM Metadata
Created in ArcGIS for the item2018-03-15 13:39:33
Last modified in ArcGIS for the item2018-03-13 16:02:12
Automatic updates

Have been performedYes
Last update2018-03-13 16:02:12

Published to an ArcIMS Metadata ServicePublished

Hide Metadata Details ▲

## Metadata Contacts ▼►

Metadata contact

Individual's nameGIS Service Center
Organization's nameCalifornia Department of Fish and Game
Contact's rolepoint of contact

Contact information ▼►

Address

e-mail address geodata@dfg.ca.gov

Hide Contact information ▲

Hide Metadata Contacts ▲

## Thumbnail and Enclosures ▼►

Thumbnail

Enclosure

Enclosure typeFile
Description of enclosureoriginal metadata
Original metadata document, which was translatedyes
Source metadata formatfgdc

Hide Thumbnail and Enclosures ▲

## FGDC Metadata (read-only) ▼►

## Identification ▼►

  Citation
    Citation Information
      Originator U.S. Geological Survey
      Originator California Department of Forestry and Fire Protection
      Publication Date Unknown
      Title
        Public Land Survey System (All Areas Filled, Includes Protracted Data) (100K Source)
      Geospatial Data Presentation Form vector digital data
      Online Linkage \\Molib01\GIS_Library\land_ownership\plss\plss_100k\pls_full
  Description
    Abstract

                                      This layer differs from the standard Public Land Survey System layer in that all landgrants and other areas excluded from the section survey process are filled in (with protracted data).  The primary purpose of this is to facilitate the georeferencing of phenomena that are spatially referenced by meridian, township, range, and section.  Though these sections do not legally exist, field personnel will interpolate to determine what the section would be if there were legally a section there.  This is common with fire starts as reported by the California Department of Forestry (CDF).  In fact, all of the work to fill in these excluded areas was completed by CDF to help georeference fire starts so they could be analyzed with GIS (Geographic Information Systems) technology.

          This layer is based on 1:100,000-scale (100K) source data.  Caution should be used when attempting to use it with more detailed sources such as 1:24,000-scale (24K) data.  For the most current and detailed PLSS data, users should refer to BLM's Geographic Coordinate Data Base (GCDB).

          This layer depicts the township, range and sections contained in the Public Land Survey System grid for the State of California. Townships are roughly six miles square, and are numbered north and south from an established baseline. Likewise, ranges are numbered east and west from an established meridian. California uses three baseline/meridians, these being Humboldt, Mt. Diablo, and San Bernardino, abbreviated H, M, and S

          Meridian, township, range, and section values are combined in the redefined item MTRS to facilitate relates from/to other tables.

    Purpose

                                      To display and analyze township, range, and sections as contained in the Public Land Survey System grid.

    Supplemental Information

                                      Converted to California Teale Albers NAD83 by the California Department of Fish and Game.  Coordinate values also converted to NAD83.

  Time Period of Content
    Time Period Information
      Single Date/Time
  Status
    Progress Complete
    Maintenance and Update Frequency None planned
  Spatial Domain
    Bounding Coordinates
      West Bounding Coordinate -124.506055
      East Bounding Coordinate -113.498654
      North Bounding Coordinate 42.068938
      South Bounding Coordinate 32.423519
  Keywords
    Theme
      Theme Keyword Thesaurus none
      Theme Keyword Public Land Survey System
      Theme Keyword ranges
      Theme Keyword townships
      Theme Keyword sections
      Theme Keyword grids
      Theme Keyword landgrants
      Theme Keyword boundaries
      Theme Keyword planningCadastre
      Theme Keyword PLS
      Theme Keyword PLSS
      Theme Keyword TRS
    Place
      Place Keyword Thesaurus none
      Place Keyword California
  Access Constraints

                                none

  Use Constraints

                                none

  Native Data Set Environment
    Microsoft Windows 2000 Version 5.2 (Build 3790) Service Pack 1; ESRI ArcCatalog 9.2.2.1350

Hide Identification ▲

## Data Quality ▼►

  Lineage
    Process Step
      Process Description

                                            Metadata edited, noted protracted nature of data.

      Process Date 2006
      Process Contact
        Contact Information
          Contact Person Primary
            Contact Person Will Patterson
            Contact Organization California Department of Fish and Game
          Contact Electronic Mail Address geodata@dfg.ca.gov
    Process Step
      Process Description

                                            Misc. edits:  32 features had Township values with control characters as the first character, followed by "06N" - changed to just "06N".  10 features had Township values of "O2N" rather than "02N" - changed to "02N".  7 features had Range values with control characters as the first character, followed by "01W" - changed to "01W".  12 features had Range values "9E" - changed to "09E".

      Process Date 2006-09
      Process Contact
        Contact Information
          Contact Person Primary
            Contact Person Joe Vondracek
            Contact Organization California Department of Fish and Game
          Contact Electronic Mail Address jvondracek@dfg.ca.gov
    Process Step
      Process Description

                                            Metadata changes.  Noted data as 100K source and added advisory about using BLM GCDB as a more detailed and current PLSS data source.

      Process Date 2007-07
      Process Contact
        Contact Information
          Contact Person Primary
            Contact Person Will Patterson
            Contact Organization California Department of Fish and Game
          Contact Electronic Mail Address geodata@dfg.ca.gov
    Process Step
      Process Description

                                            Dataset moved.

      Source Used Citation Abbreviation
        s:\land_ownership\plss\pls_full

Hide Data Quality ▲

## Spatial Reference ▼►

  Horizontal Coordinate System Definition
    Planar
      Planar Coordinate Information
        Planar Coordinate Encoding Method coordinate pair
        Coordinate Representation
          Abscissa Resolution 0.000000
          Ordinate Resolution 0.000000
        Planar Distance Units meters
    Geodetic Model
      Horizontal Datum Name North American Datum of 1983
      Ellipsoid Name Geodetic Reference System 80
      Semi-major Axis 6378137.000000
      Denominator of Flattening Ratio 298.257222

Hide Spatial Reference ▲

## Entities and Attributes ▼►

  Detailed Description
    Entity Type
      Entity Type Label PLSS_Full_100k
    Attribute
      Attribute Label FID
      Attribute Definition
        Internal feature number.
      Attribute Definition Source Esri
      Attribute Domain Values
        Unrepresentable Domain
          Sequential unique whole numbers that are automatically generated.
    Attribute
      Attribute Label Shape
      Attribute Definition
        Feature geometry.
      Attribute Definition Source ESRI
      Attribute Domain Values
        Unrepresentable Domain
          Coordinates defining the features.
    Attribute
      Attribute Label AREA
      Attribute Definition
        Area of feature in internal units squared.
      Attribute Definition Source ESRI
      Attribute Domain Values
        Unrepresentable Domain
          Positive real numbers that are automatically generated.
    Attribute
      Attribute Label PERIMETER
      Attribute Definition
        Perimeter of feature in internal units.
      Attribute Definition Source ESRI
      Attribute Domain Values
        Unrepresentable Domain
          Positive real numbers that are automatically generated.
    Attribute
      Attribute Label PLS_FULL_
    Attribute
      Attribute Label PLS_FULL_I
    Attribute
      Attribute Label MER
    Attribute
      Attribute Label TOWNSHIP
    Attribute
      Attribute Label RANGE
    Attribute
      Attribute Label SECTION
    Attribute
      Attribute Label XALB
    Attribute
      Attribute Label YALB
    Attribute
      Attribute Label LATITUDE
    Attribute
      Attribute Label LONGITUDE
    Attribute
      Attribute Label MTRS
    Attribute
      Attribute Label MTR
    Attribute
      Attribute Label Shape_Leng
    Attribute
      Attribute Label Shape_Area
      Attribute Definition
        Area of feature in internal units squared.
      Attribute Definition Source Esri
      Attribute Domain Values
        Unrepresentable Domain
          Positive real numbers that are automatically generated.

Hide Entities and Attributes ▲

## Distribution Information ▼►

  Resource Description Downloadable Data
  Standard Order Process
    Digital Form
      Digital Transfer Information
        Transfer Size 72.125

Hide Distribution Information ▲

## Metadata Reference ▼►

  Metadata Date 2007-12-07
  Metadata Contact
    Contact Information
      Contact Organization Primary
        Contact Organization California Department of Fish and Game
        Contact Person GIS Service Center
      Contact Address
      Contact Electronic Mail Address geodata@dfg.ca.gov
  Metadata Standard Name FGDC Content Standards for Digital Geospatial Metadata
  Metadata Standard Version FGDC-STD-001-1998
  Metadata Time Convention local time

Hide Metadata Reference ▲